**QCM Box 1 of 1**

1. Gamry eQCM
   1. 1 electronic 10M QCM unit
   2. 1 power supply
   3. 1 power cord
2. BNC to QCM cable
3. Cable with banana plug on each end
4. Static eQCM cell
   1. 3 white Teflon pieces of cell
   2. 4 screws for cell
   3. 2 black o-rings
   4. extra black o-rings
5. Flow eQCM Cell
   1. 1 top piece
   2. 1 bottom piece
   3. 1 base
   4. 2 screws for cell
   5. 2 clear o-rings
   6. 1 metal tube counter electrode
   7. 1 teflon plug with counter electrode (for use on static side or cell)
   8. Teflon tubing
   9. Bag of 1/8” peek finger tight tube fitting nuts
6. 2 New EQCM crystals (not for user use)
7. 1 Used EQCM crystals
8. 1 electrical adaptor for QCM crystal
9. Cables for connection pstat to 10M
   1. 1 double banana cable
   2. 1 single banana cable (use only one cable)